CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.2/conf/instr/spect/uxnmr.info
Date         : Wed May 13 08:52:44 2015
Release      : TOPSPIN Version 3.2-pl6
Installed in : C:/Bruker/TopSpin3.2
Host         : B10051821
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 2533 MHz)
User         : nmrsu
Description  : Avance III 600
Location     : University Alabama, Birmingham / USA
System       : Avance III NMR spectrometer
1H-frequency : 600.17 MHz
Order Number : 10051821
Configured in: C:/Bruker/TopSpin3.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
- Tctrl : 1
- Fctrls: 3
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/02852 ECL 06.02
- TCP/IP address = 149.236.99.89
- Firmware Version = 131205
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x43   0x5    CD  R  0.0 REC-1  AQS RXAD/2 600 Z130588/32 ECL 00.00
     3   0x34 0xd6   0x1        X  2.0 REF-1  REF/3-600 Reference Board for AQS/3 Receiver
     4   0x24 0x32     0        S  1.1 SGU-1  AQS SGU/3 600 (2CH) Z117129/00069 ECL 01.01 FPGA-Vs=20131031
     5   0x26 0x32     0        S  1.1 SGU-2  AQS SGU/3 600 (2CH) Z117129/00099 ECL 01.01 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.0 PS-1   
    14   0xa1 0x91     0        V  1.1 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0518 W1345093/0518 ECL 12:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0518 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/1936 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/6413 ECL 50
BLA_W1345096_0854 W1345096/0854 ECL 30:
- TCP/IP address = 149.236.99.251
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ INR: W1345096/0854 ECL 30
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1448 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/6400 ECL 50
LTRX Z109890/00268 ECL 02.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00268 ECL 02.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20130627
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00268 ECL 02.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/00856 ECL 03.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/00989 ECL 01.03

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.254:/dev/tty04
- Capacity: 24 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 2 s
- Sample Rail fast changer mode = no

Cryo Controller CRCO: device connected to 149.236.99.254:/dev/tty01

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.4%/0.2deg, reflection meter)
                 PN=Z103205, SN=00103 from 20120419
    Module  2 : 2H
                 PN=Z003473, SN=00918 from 20120418
    Module  3 : XBB19F 2HS
                 PN=Z003506, SN=01086 from 20120413
    Module  4 : 13C
                 PN=Z003524, SN=00417 from 20080408
    Module  5 : 15N
                 PN=Z003530, SN=00309 from 20080428


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0854 at TCP/IP 149.236.99.251)
SGU1 AUX  output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0518 at TCP/IP 149.236.99.252)
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0854 at TCP/IP 149.236.99.251)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 4 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0854 at TCP/IP 149.236.99.251)
SGU3 AUX  output -> input 2 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0518 at TCP/IP 149.236.99.252)

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0518 at TCP/IP 149.236.99.252) amplifier X-500W uses blanking 3
transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0854 at TCP/IP 149.236.99.251) amplifier 1H-100W uses blanking 2
transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0854 at TCP/IP 149.236.99.251) amplifier X-300W uses blanking 1
transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0854 at TCP/IP 149.236.99.251) amplifier 2H-150W uses blanking 4
transmitter 3 (BSMS/2 LOCK TRANSCEIVER 600 Z109890/00268 at TCP/IP 149.236.99.20) amplifier 2H-5W needs no blanking

